## ABS Components

#### General Troubleshooting Information (cont'd)

19-58

How to Retrieve ABS DTCs (KK, KX Models) Honda PGM Tester Method:

1. With the ignition switch OFF, connect the Honda PGM Tester (A) to the 16P Data Link Connector (DLC) (B) under the driver's side of the dashboard.

2. Turn the ignition switch ON (II) and follow the prompts on the PGM Tester to display the DTC (s) on the screen. After determining the DTC, refer to the DTC Troubleshooting Index.

NOTE: See the Honda PGM Tester user's manual for specific instructions.

DLC Terminal Box Method:

1. With the ignition switch OFF, connect the DLC terminal box (A) to the 16P Data Link Connector (DLC) (B) under the driver's side of the dashboard.

2. Insert the plugs of the jumper wire (C) to No. 1 and No. 12 plug holes of the DLC terminal box, then push the switch.
3. Turn the ignition switch ON (II).