## Cylinder Head

#### Timing Pulleys Installation (cont'd)

6-14

1. Tighten bolt to the specified torque using the special tool (A) (5-8840-7008-0).

Tightening torque: 196 Nm (20.0 kgf/m, 145 lbf/ft)

Oil Pump Pulley Installation

1. Install oil pump pulley (A) to oil pump shaft correctly. Tighten fastening nut to the specified torque.

Tightening torque: 44 Nm (4.5 kgf/m, 32.5 lbf/ft)

Idle Pulley Installation

1. Install the idle pulley.

Tightening torque: 80 Nm (8.2 kgf/m, 59 lbf/ft)

Fuel Supply Pump Pulley Installation

1. Install the fuel supply pump pulley (A).

Lock fuel supply pump pulley using TDC fixing bolt (B). Tighten fastening nut to the specified torque.

Tightening torque: 69 Nm (7.0 kgf/m, 50.6 lbf/ft)

a a a