## Power Windows

#### Passenger's Window Motor Test

22-198

1. Remove the passenger's door panel (see page 20-7).

2. Disconnect the 2P connector (A) from the passenger's power window motor.

   Terminal side of male terminals

3. Test the motor in each direction by connecting battery power and ground according to the table.When the motor stops running, disconnect one lead immediately.

4. If the motor does not run or fails to run smoothly, replace it.