## Rear Side Outer Panel

#### Removal

3-59

- Cut and pry off the rear side sill outer panel.
- Check the rear pillar gutter lower and gutter upper position and for damage and if necessary, replace the rear pillar gutter lower.

  1. WHEEL ARCH EXTENSION
  2. QUARTER PILLAR INNER
  3. REAR PILLAR INNER
  4. REAR PILLAR GUTTER UPPER
  5. REAR PILLAR GUTTER LOWER
  6. REAR INNER PANEL
  7. REAR PILLAR GUTTER LOWER
  8. REAR PANEL
  9. REAR PILLAR GUTTER UPPER
  10. REAR PANEL GUSSET
  11. VIEW (Z)
  12. REAR GUTTER LOWER STIFFENER
  13. OUTER PANEL