## Doors

#### Door Outer Handle Replacement

20-6

NOTE: Put on gloves to protect your hands.

1. Raise the glass fully.
2. Remove these items:

- Door panel (see page 20-4)
- Plastic cover, as necessary (see page 20-2)

3. Pull the glass run channel (A) away as necessary and remove the bolt, then remove the centre lower channel (B) by pulling it downward.

Fastener Locations

: Bolt, 1

4. On driver's and some passenger's: Release the retainer clip (A), then remove the lock cylinder (B). Disconnect the cylinder rod (C).

5. With cylinder switch: Remove the screw, then separate the lock cylinder (A) and cylinder switch (B).

Fastener Locations

: Screw, 1

a a a