## Shafts and Clutches

#### Sub-shaft Disassembly, Inspection and Reassembly

14-201

1. Remove the 1st gear (see page 14-202).

   1. 1ST GEAR
   2. LOCK NUT (FLANGE NUT)

      19 x 1.25 mm, 93 Nm (9.5 kgf/m, 69 lbf/ft), Replace

   3. CONICAL SPRING WASHER

      Replace

   4. 1ST-HOLD CLUTCH
   5. O-RING, Replace
   6. THRUST WASHER
   7. THRUST NEEDLE BEARING
   8. NEEDLE BEARING
   9. 4TH GEAR
   10. THRUST NEEDLE BEARING
   11. 4TH GEAR COLLAR
   12. NEEDLE BEARING
   13. NEEDLE BEARING STOP
   14. ATF GUIDE CAP, Replace
   15. SUB-SHAFT

2. Lubricate all parts with ATF during assembly.
3. Inspect the thrust needle bearing and the needle bearing for galling and rough movement.
4. Inspect the splines for excessive wear and damage.
5. Check shaft bearing surfaces for scoring and excessive wear.
6. Before installing the O-rings, wrap the shaft splines with tape to prevent O-ring damage.
7. Install the 1st gear and conical spring washer in the direction shown.