## Automatic Transmission

#### Shift Lever Installation (cont'd)

14-141

5-door Model

1. Cover around the opening of the console with tape or equivalent to prevent damage to the console.
2. Install the shift lever assembly (A) in the console and secure it with the bolts (B).

3. Install the bracket (C).
4. Connect the shift lock solenoid connector (D) and install it on its connector bracket.
5. Turn the ignition switch ON (II) and verify that the position indicator light comes on.

6. If necessary, push down the shift cable until it stops, then release your hand. Pull the shift cable back 1 step so that the shift cable is in

7. Turn the ignition switch OFF.
8. Rotate the socket holder (A) on the shift cable (B) counter-clockwise a quarter turn; the projection (C) on the socket holder is directed opposite the opening (D) of the shift lever bracket base (E).

Slide the holder to the shift cable bracket base and rotate the holder clockwise a quarter turn to secure the shift cable.

NOTE: Do not install the shift cable by twisting the shift cable guide (F).