## Manual Transmission

#### Input Shaft Reassembly (cont'd)

13-22

Special Tools Required

- Bearing installer 5-8840-0054-0 (J-33374)

NOTE: The insert spring set positions differ for right and left. The ends of the insert spring should not interfere with the hub.

1. Install the 3rd gear needle bearing, input 3rd gear, 3rd block ring, 3rd/4th synchroniser assembly and 4th gear needle bearing collar on the input shaft.

   NOTE:

- Be careful not to twist the inserts in the block ring opening portions when pressing.
- Note the installation direction when assembling the synchroniser assembly.

1. Using the special tool with a press the 3rd/4th synchroniser assembly (A) and 4th gear needle bearing collar (B).

1. Install the 4th block ring.

1. Install the 4th gear needle bearing.

1. Install the input 4th gear.

1. Install the 4th gear thrust washer. Note the installation direction.

1. Install the rear input shaft bearing (A). Using the special tool, press the bearing into place.

1. Install the input shaft bearing (A). Using the special tool, press the bearing into place.

a a a