## Frame

#### Frame Repair Chart (cont'd)

20-135

m | Locating holes Ø25 (0.98) | u | For upper arm bracket centre Ø15 (0.59)
n | For trailing arm Ø13 (0.51) | v1, v2 | Locating hole Ø13 (0.51)
o | Locating holes Ø25 (0.98) | w | For upper arm Ø13 (0.51)
p | Locating holes Ø20 (0.79) | x | For lower arm centre
q | Trailing arm centre | y | Locating hole Ø50 (1.97)
r | Rear damper centre 73 x 68 (Slot) | z | Locating hole Ø20 (0.79)
s | For upper arm Ø13 (0.51) |  |
t | For trailing arm Ø13 (0.51) |  |