## Interior Trim

#### Trim Removal/Installation - Trunk Area

20-67

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown.

Install the trim in the reverse order of removal, and replace any damaged clips.

Fastener Locations
A : Clip, 4 | B : Clip, 4 | C: Clip, 7 or 8

1. LEFT TRUNK SIDE TRIM PANEL
2. SPARE TYRE LID
3. TRUNK FLOOR MAT
4. Folding type rear seat only
5. LEFT TRUNK SIDE TRIM PANEL
6. RIGHT TRUNK SIDE TRIM PANEL
7. SPARE TYRE LID

   (Without trunk floor spacer)

8. RIGHT TRUNK FLOOR SIDE SPACER
9. RIGHT TRUNK SIDE TRIM PANEL
10. TRUNK FLOOR CENTRE SPACER
11. TRUNK REAR TRIM PANEL
12. LEFT TRUNK FLOOR SIDE SPACER