## Driveline/Axle

#### Driveshaft Reassembly

16-9

Exploded View

Japan produced models:

1. SET RING

   Replace.

2. INBOARD JOINT
3. CIRCLIP
4. ROLLER
5. SPIDER
6. INBOARD BOOT

   Pack cavity with grease.

7. DOUBLE LOOP BAND

   Replace.

8. Pack cavity with grease.
9. Left driveshaft
10. DYNAMIC DAMPER BAND

    Replace.

11. DRIVESHAFT
12. STOP RING

    Replace.

13. BOOT BANDS

    Replace.

14. OUTBOARD JOINT
15. Pack cavity with grease.
16. OUTBOARD BOOT (TYPE)
17. Right driveshaft

    (Except SOHC engine A/T models)

18. DYNAMIC DAMPER

    (Undirectional)