## Power Mirrors

#### Power Mirror Actuator Replacement (cont'd)

22-150

9. Route the wire harness (A) of the new actuator through the hole in the bracket (B).

10. Insert the new actuator terminals into the connector in the original arrangement as shown below.

Terminal side of male terminals

*1: With defogger

*2: With retract mirror

11. Reassemble the mirror in the reverse order of disassembly. Be careful not to break in the mirror holder when installing it to the actuator.
12. After installing, check the power mirror operation.

5-door:

1. Remove the mirror holder the power mirror (see page 20-170).
2. Remove the power mirror (see page 20-170) and disconnect the connector.
3. Remove the cover (A) and screw from the mirror connector (B).

4. Record the terminal locations and wire colours.
5. Cut the wire harness with the wire cutter.
6. Remove the three mounting screws and separate the mirror housing (A) from the bracket (B).