## PGM-FI System

#### DTC Troubleshooting (cont'd)

11-243

10. Disconnect ECM/PCM connector B (24P).

11. Check for continuity between ECM/PCM connector terminal B15 and body ground.

ECM/PCM CONNECTOR B (24P)

Wire side of female terminals

Is there continuity?

YES | - Repair short in the wire between the VTEC solenoid valve and the ECM/PCM (B15).
NO | - Go to step 12.

12. Connect the VTEC solenoid valve 1P (2P)* connector terminal No. 1 and body ground with a jumper wire.

VTEC SOLENOID VALVE HARNESS CONNECTORS

Wire side of female terminal

Wire side of female terminal

13. Check for continuity between ECM/PCM connector terminal B15 and body ground.

ECM/PCM CONNECTOR B (24P)

Wire side of female terminals

Is there continuity?

YES | - Go to step 14.
NO | - Repair short in the wire between the VTEC solenoid valve and the ECM/PCM (B15).