## Exterior Trim

#### Rear License Trim Replacement

20-255

NOTE: Put on gloves to protect your hands.

1. Remove the tailgate lower trim panel (see page 20-209).
2. On inside the tailgate, remove the bolts securing the rear license trim (A) and tailgate lock cylinder (B).

   Fastener Locations
   : Bolt, 2

3. From inside the tailgate, release the clips (A, B) while holding the rear license trim (C), then remove the trim. Take care not to scratch the tailgate.

Fastener Locations
A : Clip, 2 | B : Clip, 2

4. Install the trim in the reverse order of removal and replace any damaged clips.