## Design Specifications

#### (cont'd)

2-9

Item | Measurement | Qualification | Specification
CLUTCH | Clutch |  | Single plate dry, diaphragm spring
MANUAL TRANSMISSION | Type |  | Synchronised, 5-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.545
2nd | 2.055
3rd | 1.333
4th | 0.923
5th | 0.744
Reverse | 3.583
Final reduction | Type | Single helical gear
Gear ratio | 3.578
STEERING | Type |  | Rack and pinion, with electrical power assistance
Over ratio |  | 14.49
Turns, lock-to-lock |  | 2.83
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type | Front | Strut
Rear | Double wishbone
Shock absorber | Front and rear | Telescopic, hydraulic, nitrogen gas-filled
WHEEL ALIGNMENT | Camber | Front | 0°
Rear | – 0°45'
Caster | Front | 1°33'
Total toe | Front | 0 mm (0 in.)
Rear | In 2 mm (1/16 in.)
BRAKES | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid disc
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 40 cm2 x 2 (6.3 sq in. x 2)
Rear | 28 cm2x 2 (4.3 sq in. x 2)
TYRES | Size of front and rear |  | 195/60R15 88H
Size of spare |  | T125/70D15 95M
AIR CONDITIONING | Cooling capacity |  | 3,612 kcal/h (14,370 BTU/h)
Compressor | Type/manufacturer | Swash plate/DELPHI
Number of cylinders | 6
Capacity | 135 ml/rev. (5.23 cu in./rev.)
Maximum speed | 8,000 rpm
Lubricant capacity | 150 ml (5 fl oz)
Lubricant type | DH-PS
Condenser | Type | Multi flow
Evaporator | Type | Laminate
Blower | Type | Sirocco fan
Motor type | 220 W/12 V
Speed control | 9-speed
Maximum capacity | 470 m3/h (16,900 cu ft/h)
Temperature clutch |  | Air-mix type
Compressor clutch | Type | Dry, single plate, poly-V belt drive
Refrigerant | Type | HFC-134a (R-134a)
Quantity | 500 – 550 g (17.5 – 19.5 oz)

a a a