## Honda Multi Matic Transmission/CVT

#### Shift Cable Replacement (cont'd)

14-344

8. Remove the spring clip (A), washer (B) and plastic washer (C) from the control lever (D).

9. Loosen the locknut, then remove the shift cable (E).
10. Insert the new shift cable through the grommet hole, then install the shift cable guide brackets and grommet.
11. Verify that the transmission is in position on the control lever.
12. Align the socket on the shift cable with the slot in the shift cable bracket, then install the socket in the bracket and shift cable end to the control lever. Do not bend the shift cable excessively.
13. Tighten the locknut.
14. Install the plastic washer then the steel washer and install the spring clip (H) in the direction shown.
15. Install the heat shield and the exhaust pipe A, then connect the secondary HO2S connector.

16. Turn the ignition switch ON (II) and verify that the position indicator light comes on.

17. If necessary, push the shift cable until it stops, then release your hand. Pull the shift cable back two steps so that the shift position is in

18. Turn the ignition switch OFF.
19. Insert a 6.0 mm (0.24 in.) pin (A) through the positioning hole (B) on the shift lever bracket base and into the positioning hole (C) on the shift lever assembly.