## Power Mirrors

#### Power Mirror Actuator Replacement (cont'd)

22-12

8. Insert the terminal into the connector as shown below:

9. Seal the intersection of wire harness with tape.
10. Reassemble in the reverse order of disassembly. Be careful not to break the mirror when reinstalling into the actuator.
11. Reinstall the mirror assembly onto the door.
12. Operate the power mirror to ensure smooth operation.

a a a