## Engine Assembly

#### Engine Removal (cont'd)

5-4

1. Remove the battery cables (A) from the under-hood fuse/relay box, then remove the harness clamp (B) and ground cable (C).

1. Fully open the throttle link by hand, then remove the throttle cable (A) from the link. Loosen the lockout (B) and remove the cable from the bracket.

1. Disconnect the Engine Control Module (ECM) connectors (A) and main wire harness connector (B).

LHD models:

RHD models:

a a a