## Power Windows

#### Passenger's Window Switch Test

22-195

1. Remove the passenger's power window switch (A) (see page 22-201).

2. Disconnect the 20P connector from the switch.

3. Check for continuity between the terminals in each switch position according to the table.

Front Passenger's (LHD type):

Front Passenger's (RHD type):

Left Rear Window:

Right Rear Window:

[ ] : 5 door

4. If the switch is faulty, replace the switch.