## Driveline/Axle

#### Driveshafts Reassembly

16-11

Exploded View

1. SET RING

   Replace.

2. INBOARD JOINT
3. CIRCLIP
4. SPIDER AND ROLLERS
5. DOUBLE LOOP BAND

   Replace.

   (Replacement parts only)

6. INBOARD BOOT

   Pack cavity with grease

7. EAR CLAMP BAND

   Replace.

8. LOW PROFILE BAND

   Replace.

9. Pack cavity with grease
10. EAR CLAMP BAND

    Replace.

11. DRIVESHAFT
12. STOP RING

    Replace.

13. EAR CLAMP BANDS

    Replace.

14. OUTBOARD JOINT
15. Pack cavity with grease
16. OUTBOARD BOOT
17. DYNAMIC DAMPER

a a a