## Doors

#### Door Outer Handle Replacement (cont'd)

20-6

5. With cylinder switch: Disconnect the cylinder switch connector (A) and detach the harness clips (B), then remove the cylinder switch (C).

6. Pull the glass run channel (A) away as necessary.

7. Remove the maintenance hole (A). Disconnect the outer handle rod (B) and remove the nuts, then remove the outer handle protector (C) from the outer handle (D).

Fastener Locations

: Nut, 2

8. Pull out the outer handle (A) in the numbered sequence and remove it.