## Automatic Transmission

#### Pressure Tests

14-114

Special Tools Required

A/T oil pressure gauge set, 07406-0020004

1. Before testing, be sure the transmission fluid is filled to the proper level.
2. Raise the front of the vehicle and make sure it is securely supported.
3. Set the parking brake and block rear wheels securely.
4. Allow the front wheels to rotate freely.
5. Warm up the engine (the radiator fan comes on), then stop it and connect the tachometer.
6. Connect the oil pressure gauges to each inspection hole and do not allow dust or other foreign particles to enter the holes while connecting the gauges.

   TORQUE: 18 Nm (1.8 kgf/m, 13 lbf/ft)

   1. A/T OIL PRESSURE GAUGE SET

      07406-0020004

   2. A

      LINE PRESSURE INSPECTION HOLE

   3. F

      1ST-HOLD CLUTCH PRESSURE INSPECTION HOLE

      (7-position transmission)

   4. E

      4TH CLUTCH PRESSURE INSPECTION HOLE

   5. B

      1ST CLUTCH PRESSURE INSPECTION HOLE

   6. D

      3RD CLUTCH PRESSURE INSPECTION HOLE

   7. C

      2ND CLUTCH PRESSURE INSPECTION HOLE