## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-130

DTC 15-1: Faulty OPDS Unit

1. Make sure nothing is sitting on the front passenger's seat.
2. Initialise the OPDS unit (see page 23-39).
3. Erase the DTC memory (see page 23-38).
4. Read the DTC.

Is DTC 15-1 indicated?

YES - Go to step 5.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

5. Check the No. 9 (10A) fuse in the under-dash fuse/relay box.

Is the fuse OK?

YES - Go to step 6.

NO - Go to step 9.

6. Disconnect the O1i connector (A) from the OPDS unit (B).

7. Turn the ignition switch ON (II).

8. Check for voltage between the No. 4 terminal of the O1i connector and body ground. There should be battery voltage.

O1i CONNECTOR

Wire side of female terminals

Is there battery voltage?

YES - Go to step 16.

NO - Open in the floor wire harness or in the OPDS unit harness; replace the faulty harness.

9. Replace the No. 9 (10A) fuse in the under-dash fuse/relay box.
10. Turn the ignition switch ON (II) for 30 seconds then turn it OFF.
11. Check the No. 9 (10A) fuse in under-dash fuse/relay box.

Is the fuse OK?

YES - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

NO - Go to step 12.

12. Replace the No. 9 (10 A) fuse in the under-dash fuse/relay box.