## Forward Clutch

#### Clutch Disassembly

14-366

Special Tools Required

- Clutch spring compressor set, 07LAE-PX40000
  - Clutch spring compressor attachment, 07LAE-PX40100
  - Clutch spring compressor attachment, 07HAE-PL50101
  - Clutch spring compressor bolt assembly, 07GAE-PG40200

- Snap ring pliers, 07LGC-0010100

1. Remove the snap ring (A), then remove the clutch end plate, the clutch discs and the plates with a screwdriver (B).

2. Remove the disc spring.

3. Install the special tool on the clutch assembly.

4. Be sure the special tool (A) is adjusted to have full contact with the spring retainer (B) on the clutch.