## EPS Components

#### DTC Troubleshooting (cont'd)

17-75

7. Turn the ignition switch ON (II).

8. Measure the voltage between the EPS control unit connector C (20P) terminal No. 15 and body ground.

   EPS CONTROL UNIT CONNECTOR C (20P)

Wire side of female terminals

Is there battery voltage?

YES - Repair short to power in the + circuit wire between the torque sensor and EPS control unit.

NO - Go to step 9.

9. Turn the ignition switch OFF.

10. Check for continuity between the EPS control unit connector C (20P) terminal No. 15 and the torque sensor 6P connector terminal No. 4.

EPS CONTROL UNIT CONNECTOR C (20P)

Wire side of female terminals

Is there continuity?

YES - Go to step 11.

NO - Repair open in the wire between the torque sensor and the EPS control unit.