## Sunroof

#### Symptom Troubleshooting Index

20-51

Symptom | Diagnostic procedure | Also check for
Water leaks |

1. Check for a clogged drain tube.
2. Check for a gap between the glass weatherstrip and the roof panel.
3. Check for a defective or an improperly installed glass weatherstrip or drain channel.
4. Check for a gap between the drain seal and the roof panel.

Wind noise |

1. Check for excessive clearance between the glass weatherstrip and the roof panel.

Motor noise |

1. Check for a loose motor.
2. Check for a worn gear or bearing.
3. Check for a deformed cable assembly.

Glass does not move, but motor turns |

1. Check for a defective gear or inner cable.
2. Check for foreign matter stuck between the guide rail and the slider.
3. Check for a loose inner cable.
4. Make sure the cable assembly is attached properly.

Glass does not move and motor does not turn (glass can be moved with sunroof wrench) |

1. Check for a blown fuse.
2. Check for a faulty sunroof switch.
3. Check the limit switch.
4. Check for a run down battery.
5. Check for a defective motor.
6. Check for a faulty relay.