## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-117

6. Reconnect the battery negative cable.

7. Erase the DTC memory.
8. Read the DTC.

Is DTC 12-5 indicated?

YES - Go to step 9.

NO - Short to ground in the right side airbag inflator, replace the right side airbag.

9. Disconnect the battery negative cable and wait for 3 minutes.
10. Disconnect the SLi connector (A) from the left side airbag (B).

11. Disconnect the U2o connector (A) from the SRS unit (B).

12. Check resistance between the No. 15 and No. 18 terminals of the U2o connector, and between the No. 16 and No. 18 terminals of the U2o connector. Then check resistance between the No. 18 terminal of the U2o connector and body ground. There should be 1 M ohm or more.

U2o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty SRS unit; replace the SRS unit.

NO - Short to ground in the floor wire harness; replace the floor wire harness.