## Conventional Brake Components

#### Parking Brake Switch Test

19-10
Brake Fluid Level Switch Test

1. Remove the console and disconnect the connector (A) from the switch (B).

2. Check for continuity between the positive terminal and body ground:

- With the brake lever up, there should be continuity.
- With the brake lever down, there should be no continuity.

Check for continuity between the terminals (A) with the float in the down position and the up position

- Remove the brake fluid completely from the reservoir.
  With the float down, there should be continuity.
- File the reservoir with brake fluid to MAX (upper) level (B). With the float up, there should be no continuity.

4-door:

5-door: