## Standards and Service Limits

#### Engine Electrical (cont'd)

2-3

Item | Measurement | Qualification | Standard or New | Service Limit
Starter (4-door and 5-door (Japan made) models) for D15Y2, D16W7 (KG model), D16W8, D17Z1 (Except Malaysia model), D17A1, D17A2 (Except Malaysia model), D17A5 (Except Indonesia model) engines (DENSO) | Output |  | 1.0 kW
Commutator mica depth |  | 0.50-0.75 mm (0.020-0.030 in.) | 0.2 mm (0.008 in)
Commutator runout |  | 0.02 mm (0.001 in.) max. | 0.05 mm (0.002 in)
Commutator O.D. |  | 27.9-28.0 mm (1.098-1.102 in.) | 27.0 mm (1.063 in.)
Brush length |  | 14.0-14.5 mm (0.55-0.57 in.) | 9.0 mm (0.35 in)
Brush spring tension |  | 13.7-17.7 N (1.4-1.8 kgf, 3.09-4.00 lbf) |
Starter (4-door and 5-door (Japan made) models) for D15Y3 (Philippine model), D16W9 (Philippine model), D17Z1 (Malaysia model), D17Z5, D17A2 (Malaysia model), D17A5 (Indonesia model) engines (MITSUBISHI) | Output |  | 0.8 kW
Commutator mica depth |  | 0.50-0.75 mm (0.020-0.030 in.) | 0.2 mm (0.008 in.)
Commutator runout |  | 0.05 mm (0.002 in.) max | 0.4 mm (0.02 in).
Commutator O.D. |  | 27.9-28.0 mm (1.098-1.102 in.) | 27.0 mm (1.063 in.)
Brush length |  | 9.7-10.3 mm (0.38-0.41 in.) | 6.0 mm (0.24 in)
Brush spring tension |  | 13.7-17.7 N (1.4-1.8 kgf, 3.09-4.00 lbf) |
Starter (4-door and 5-door (Japan made) models) for Except D15Y2, D15Y3 (Philippine model), D16W7 (KG model), D16W8, D16W9, D17Z1, D17A1, D17A2, D17A5 engines (DENSO) | Output |  | 0.8 kW
Commutator mica depth |  | 0.50-0.75 mm (0.020-0.030 in.) | 0.2 mm (0.008 in.)
Commutator runout |  | 0.05 mm (0.002 in.) max. | 0.4 mm (0.02 in.)
Commutator O.D. |  | 27.9-28.0 mm (1.098-1.102 in.) | 27.0 mm (1.063 in.)
Brush length |  | 9.7-10.3 mm (0.35-0.41 in.) | 6.0 mm (0.24 in.)
Starter (Coupe model) | Output |  | 1.0 kW
Commutator mica depth |  | 0.45-0.75 mm (0.018-0.030 in.) | 0.2 mm (0.008 in)
Commutator runout |  | 0.02 mm (0.001 in.) max. | 0.05 mm (0.002 in)
Commutator O.D. |  | 27.9-28.0 mm (1.098-1.102 in.) | 27.0 mm (1.063 in.)
Brush length |  | 14.0-14.3 mm (0.55-0.57 in.) | 9.0 mm (0.35 in)
Brush spring tension |  | 14.0-20.0 N (1.4-2.0 kgf, 4.00-5.30 lbf) |
Starter (5-door (England made) models) for D14Z6, D16V1 (KE model), D16V3 engines (DENSO) | Output |  | 0.8 kW
Commutator mica depth |  | 0.50-0.75 mm (0.020-0.030 in.) | 0.2 mm (0.008 in.)
Commutator runout |  | 0.05 mm (0.002 in.) max. | 0.4 mm (0.02 in.)
Commutator O.D. |  | 27.9-28.0 mm (1.098-1.102 in.) | 27.0 mm (1.063 in.)
Brush length |  | 9.7-10.3 mm (0.35-0.41 in.) | 6.0 mm (0.24 in.)

a a a