## Standards and Service Limits

#### Clutch

2-10

Item | Measurement | Qualification | Standard or New | Service Limit
Clutch pedal | Height from the floor |  | 198 mm (7.8 in.) | -
Stroke |  | 130-140 mm (5.1-5.5 in.) | -
Play |  | 8-18 mm (0.3-0.7 in.) | -
Disengagement height from the floor |  | 113 mm (4.4 in.) min. | -
Flywheel | Runout on clutch mating surface |  | 0.06 mm (0.002 in.) max. | 0.15 mm (0.006 in.)
Clutch disc | Rivet head depth | D17A engine | 1.65-2.25 mm (0.065-0.089 in.) | 0.8 mm (0.03 in.)
Except D17A engine | 1.2-1.7 mm (0.047-0.067 in.) | 0.2 mm (0.01 in.)
Thickness |  | 8.3-9.0 mm (0.33-0.35 in.) | 5.7 mm (0.22 in.)
Pressure plate | Warpage |  | 0.03 mm (0.001 in.) max. | 0.15 mm (0.006 in.)
Height of diaphragm spring fingers | Measure with feeler gauge and special tool | D16W7, D16W8, D16W9, D16V2 engines | 0.6 mm (0.02 in.) max. | 0.8 mm (0.03 in.)
Except D16W7, D16W8, D16W9, D16V2 engines | 0.6 mm (0.02 in.) max. | 1.0 mm (0.04 in.)