## Heating

#### Symptom Troubleshooting Index (cont'd)

21-9

5-door KE Model

Symptom | Diagnostic procedure | Also check for
Recirculation control doors do not change between Fresh and Recirculate | Recirculation Control Motor Circuit Troubleshooting (see page 21-35) |

- Blown fuse No. 14 (10A) in the under-dash fuse/relay box
- Cleanliness and tightness of all connectors

Both heater and A/C do not work | Heater Control Power and Ground Circuits Troubleshooting (see page 21-43) |

- Blown fuse No. 14 (10A) in the under-dash fuse/relay box
- Poor ground at G501
- Cleanliness and tightness of all connectors