## Manual Transmission

#### Transmission Disassembly (cont'd)

13-19

1. Remove the 8 mm flange bolts in a criss-cross pattern in several steps.

1. Remove the harness bracket (A), the transmission hanger A (B) and the transmission hanger B (C).

1. Remove the 32 mm sealing cap (A).

1. Expand the 72 mm snap ring (B) on the countershaft ball bearing and remove it from the groove using a pair of snap ring pliers.

1. Remove the transmission housing (C) and 14 x 20 mm dowel pins (D).

1. Remove the reverse idler gear (A) and reverse gear shaft (B).

1. Remove the reverse shift fork.

a a a