## Bumpers

#### Front Bumper Removal/Installation

20-8

NOTE:

- Have an assistant help you when removing and installing the front bumper.
- Take care not to scratch the front bumper and body.
- Put on gloves to protect your hands.

Remove the front bumper as shown.

Install the bumper in the reverse order of removal and note these items:

- If equipped, make sure the headlight washer tube is connected properly.
- Make sure the front bumper engages the hooks of the side spacers and upper beams on both sides securely.
- Replace any damaged clips.

Fastener Locations

A: Screw, 2 B : Screw, 2 C: Bolt, 4 D : Clip, 7 E : Clip, 2

1. HOOKS
2. HOOKS
3. SIDE SPACER
4. UPPER BEAM
5. FRONT INNER FENDER
6. FRONT BUMPER
7. HEADLIGHT WASHER TUBE

   (For some models)

8. FRONT AIR SPOILER
9. 6 x 1.0 mm

   9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

10. AIR SPOILER PLATE
11. PLATE
12. SPOILER
13. BUMPER