## Doors

#### Front Door Outer Handle Replacement (cont'd)

20-9

5. With cylinder switch: Disconnect the cylinder switch connector (A), and detach the harness clips (B), then remove the cylinder switch (C).

6. Disconnect the outer handle rod (A), and remove the nuts, then remove the outer handle protector (B) from the outer handle (C).

   Fastener Locations
   : Nut, 2

7. Pull out the outer handle (A) in the numbered sequence, and remove it.

8. Install the handle in the reverse order of removal, and note these items:

- Make sure the cylinder switch harness is routed properly ( for some models).
- Make sure the cylinder switch connector is plugged in properly (for some models), and each rod is connected securely.
- Make sure the door locks and opens properly.
- When installing the lock cylinder, leave the outer door handle bolts loose so the inner protector does not interfere with the lock cylinder, then tighten the handle bolts.
- Install the lock cylinder retaining clip on the handle, then install the lock cylinder. Be sure the clip is fully seated in the slot on the lock cylinder.