## Seats

#### Rear Seat Removal/Installation - Folding Type

20-95

NOTE: Take care not to scratch the body or tear the seat covers.

Remove the rear seat as shown.

Install the seat in the reverse order of removal, and note these items:

- Before attaching the rear seat-back and cushion, make sure there are no twists or kinks in the rear seat belts and centre belt.
- When installing the seat cushion, slip the seat belt buckles through the slits in the seat cushion.
- Make sure the seat-back locks securely.

  Fastener Locations
  A : Bolt, 1 | B : Bolt, 2 | C : Bolt, 2 | D : Bolt, 1
  1. HOOK
  2. HOOK

     Release it from trunk compartment

  3. HOOK
  4. PIVOT BRACKET
  5. LEFT SEAT SIDE BOLSTER
  6. BUSHING
  7. CLIP
  8. CENTRE BELT

     (For some models)

     Remove the belt from the centre belt guide.

  9. SEAT BELT BUCKLE
  10. CLIP
  11. HOOK
  12. SEAT CUSHION
  13. RIGHT SEAT-BACK
  14. RIGHT SEAT SIDE BOLSTER
  15. BUSHING
  16. BUSHING