## ABS Components

#### ABS Indicator Circuit Troubleshooting (cont'd)

19-112

9. Disconnect the gauge assembly connector B (22P), and go to step 10 for 4-door model. Disconnect the gauge assembly connector A (22P) and go to step 12 for 5-door model.

10. Check for continuity between the gauge assembly connector B (22P) terminal No. 15 and body ground.

GAUGE ASSEMBLY CONNECTOR B (22P)

Wire side of female terminals

Is there continuity?

YES - Repair short to body ground in the wire between the gauge assembly and the ABS control unit.

NO - Go to step 11.

11. Check for continuity between the gauge assembly connector B (22P) terminal No. 18 and body ground.

GAUGE ASSEMBLY CONNECTOR B (22P)

Wire side of female terminals

Is there continuity?

YES - Check for loose terminals in the gauge assembly connectors. If the connectors are OK, replace the gauge assembly.

NO - Repair open in the wire between the gauge assembly and body ground (G501).

12. Check for continuity between the gauge assembly connector A (22P) terminal No. 12 and body ground.

GAUGE ASSEMBLY CONNECTOR B (22P)

Wire side of female terminals

Is there continuity?

YES - Repair short to body ground in the wire between the gauge assembly and the ABS control unit.

NO - Go to step 13.

13. Check for continuity between the gauge assembly connector B (22P) terminal No. 12 and body ground.

GAUGE ASSEMBLY CONNECTOR B (22P)

Wire side of female terminals

Is there continuity?

YES - Check for loose terminals in the gauge assembly connectors. If the connectors are OK, replace the gauge assembly.

NO - Repair open in the wire between the gauge assembly and body ground (G501).