## Interior Trim

#### Trim Removal/Installation - Trunk Area

20-36

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown. To remove the trunk side trim panel, remove the side trim panel as necessary (see page 20-35).

Install the trim in the reverse order of removal and replace any damaged clips.

Fastener Locations

A : Clip, 4B : Clip, 2C : Clip, 6

1. LEFT TRUNK SIDE TRIM PANEL
2. SPARE TYRE LID
3. TRUNK FLOOR MAT
4. Without trunk floor spacer:
5. To body
6. HOOKS
7. HOOKS
8. To body.
9. RIGHT TRUNK FLOOR SIDE SPACER

   (For some models)

10. RIGHT TRUNK SIDE TRIM PANEL
11. TRUNK FLOOR CENTRE SPACER

    (For some models)

12. TRUNK REAR TRIM PANEL
13. LEFT TRUNK FLOOR SIDE SPACER

    (For some models)