## Power Steering

#### Steering Gearbox Overhaul

17-39

Exploded View

1. CYLINDER END SEAL

   Replace.

2. BACKUP RING
3. BUSHING

   Replace.

4. LOCK SCREW

   Replace.

   162 Nm (16.5 kgf/m, 119 lbf/ft)

5. CYLINDER LINES

   17 Nm (1.7 kgf/m, 12 lbf/ft)

6. BUSHING
7. VALVE OIL SEAL

   Replace.

8. VALVE HOUSING
9. FLANGE BOLTS

   20 Nm (2.0 kgf/m, 14 lbf/ft)

10. SNAP RING

    Replace.

11. SLEEVE
12. SLEEVE SEAL RINGS

    Replace.

13. VALVE SEAL RING

    Replace.

14. O-RING

    Replace.

15. VALVE OIL SEAL

    Replace.

16. WAVE WASHER
17. PINION SHAFT
18. O-RING

    Replace.

19. RACK GUIDE
20. SPRING
21. RACK GUIDE SCREW
22. LOCKNUT
23. GEARBOX HOUSING
24. STEERING RACK
25. SNAP RING
26. BACKUP RING
27. CYLINDER END SEAL

    Replace.

28. O-RING

    Replace.

29. PISTON SEAL RING

    Replace.

30. TIE-ROD END
31. RACK END

    54 Nm (5.5 kgf/m, 40 lbf/ft)

32. SLIDER GUIDE
33. LOCK WASHER

    Replace.

34. 12mm FLANGE BOLTS

    69 Nm (7.0 kgf/m, 51 lbf/ft)

35. STOP WASHER

    Replace.

36. O-RINGS

    Replace.

37. BRACKET
38. BOOT BAND

    Replace.

39. BOOT B
40. CLIP
41. FLANGE BOLT

    20 Nm (2.0 kgf/m, 14 lbf/ft)

42. BOOT GUARD
43. RACK END PLUG

    29 Nm (3.0 kgf/m, 22 lbf/ft)

44. BOOT BANDS

    Replace.

45. BOOT A
46. CYLINDER HOUSING
47. STOP RING, Replace