## SRS

#### DTC Troubleshooting (cont'd)

23-65

8. Read the DTC.

Is DTC 2-3 indicated?

YES - Go to step 9.

NO - Short in the front passenger's airbag inflator; replace the front passenger's airbag (see page 23-167).

9. Disconnect the battery negative cable and wait for 3 minutes.
10. Disconnect the D1o connector (A) from the D1i connector (B).

11. Disconnect the TL1o and TR1o connectors (A) from the TL1i and TR1i connectors (B).

12. Disconnect the U1o connector (A) from the SRS unit (B).

13. Disconnect the special tool (2 ohm) from the P1i connector.
14. Check resistance between the No. 5 and No. 14 terminals of the U1o connector. There should be 1 M ohm or more.

U1o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty SRS unit; replace the SRS unit (see page 23-176).

NO - Short in dashboard wire harness B; replace dashboard wire harness B.