## Dashboard

#### Dashboard Removal/Installation (cont'd)

20-83

Middle portion (LHD):

7. From the passenger's side, disconnect the floor wire harness connectors (A), engine compartment wire harness connectors (B), and A/C sub wire harness connectors (C).

8. On the driver's side, disconnect the floor wire harness connector (A) and engine compartment wire harness connector (B), and using a Torx T30 bit, remove the ground bolt (C). On AT model, disconnect the parking pin shift connector (D) and shift lock solenoid connector (E).

Middle portion (RHD):

9. From the driver's side, disconnect the floor wire harness connectors (A), engine compartment wire harness connectors (B), and A/C sub wire harness connectors (C).

10. On the passenger's side, disconnect the floor wire harness connector (A) and engine compartment wire harness connector (B), and using a Torx T30 bit, remove the ground bolt (C). On AT model, disconnect the parking pin shift connector (D) and shift lock solenoid connector (E).