## EPS Components

#### DTC Troubleshooting Index

17-68

DTC | Detection Item | Note
DTC: 12 | A problem with voltage for torque sensor T/SIG | (see page 17-74)
DTC: 16 | A problem with average of voltage for torque sensor VT3 and VT6 | (see page 17-76)
DTC: 17 | A problem with the voltage for torque sensor 12 V power source Vcc 1 | (see page 17-78)
DTC: 18 | A problem with the voltage for torque sensor 5 V power source Vcc 2 | (see page 17-78)
DTC: 22 | A problem with the average for vehicle speed and engine speed | (see page 17-80)
| Excessive change of the vehicle speed sensor signal | (see page 17-80)
DTC: 23 | A problem with the engine speed signal circuit | (see page 17-80)
DTC: 37 | A problem with the circuit for input motor voltage in the EPS control unit | (see page 17-81)
DTC: 41 | A problem with the motor voltage | (see page 17-82)
DTC: 42 | A problem with the motor driven current | (see page 17-84)
DTC: 43 | A problem with the motor driven current | (see page 17-87)
DTC: 45 | A problem with the motor driven current | (see page 17-84)
DTC: 47 | A problem with the motor relay in the EPS control unit | (see page 17-88)
DTC: 50 | A problem with the CPU in the EPS control unit | (see page 17-89)
DTC: 51 | A problem with E2PROM in the EPS control unit | (see page 17-89)
DTC: 62 | Fail-safe relay stuck ON | (see page 17-90)
DTC: 64 | A problem with low battery voltage | (see page 17-90)
| Fail-safe relay contact failure | (see page 17-90)
DTC: 66 | A problem with the motor driven voltage | (see page 17-91)
DTC: 67 | A problem with the torque sensor I/F circuit | (see page 17-91)
DTC: 68 | A problem with the interlock circuit | (see page 17-91)
DTC: 69 | A problem with the interlock circuit | (see page 17-92)