## Maintenance Schedule for Severe Conditions (Except European Models)

#### Listed by Distance/Time

3-10

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 5,000 km (3,000 miles) or 6 months
Replace engine oil filter | Every 10,000 km (6,000 miles) or 6 months
Replace air cleaner element | Every 20,000 km (12,000 miles)
Inspect valve clearance | with catalytic converter | Every 40,000 km (24,000 miles)
without catalytic converter | Every 20,000 km (12,000 miles)
Replace fuel filter |  | l |  | l |  | l |  | l |  | l
Replace spark plugs | with catalytic converter | Every 40,000 km (24,000 miles)
without catalytic converter | Every 20,000 km (12,000 miles)
Replace timing belt and inspect water pump |  |  |  |  | l |  |  |  |  | l
Inspect and adjust drive belts |  | l |  | l |  | l |  | l |  | l
Inspect idle speed | with catalytic converter |  |  |  |  |  | l |  |  |  |
without catalytic converter |  |  | l |  |  | l |  |  | l |
Replace engine coolant | 200,000 km (120,000 miles) or 120 months, thereafter every 100,000 km (60,000 miles) or 60 months
Replace transmission fluid | Manual Transmission |  |  | l |  |  | l |  |  | l |
Automatic Transmission |  |  | l |  | l |  | l |  | l |
Inspect front and rear brakes | Every 10,000 km (6,000 miles) or 6 months
Replace brake fluid | Every 36 months
Check parking brake adjustment | l | l |  | l |  | l |  | l |  | l
Rotate tyre (Check tyre inflation and condition at least once per month) | Every 10,000 km (6,000 miles)
| Visually inspect the following items:
Tie rod ends, steering gearbox and boots | Every 10,000 km (6,000 miles) or 6 months
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS) | l | l | l | l | l | l | l | l | l | l
All fluid levels and condition of fluid
Exhaust system
Fuel line and connections

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35°C (95°F) conditions.
- Extensive idling of long periods of stop-and-go-driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.