## Engine Lubrication

#### Engine Oil Replacement

8-3

1. Warm up the engine.
2. Remove the drain bolt (A) and drain the engine oil.

D14Z6, D16V1 engines:

D16V3 engine:

3. Reinstall the drain bolt with a new washer (B).

4. Refill with the recommended oil (see page 3-2).

Capacity

D14Z6, D16V1 engines:

3.3 l (3.5 US qt, 2.9 Imp qt) at oil change.

3.5 l (3.7 US qt, 3.1 Imp qt) at oil change.

including filter

4.2 l (4.4 US qt, 3.7 Imp qt) after engine overhaul.

D16V3 engine:

3.0 l (3.2 US qt, 2.6 Imp qt) at oil change.

3.2 l (3.4 US qt, 2.8 Imp qt) at oil change.

including filter

4.2 l (4.4 US qt, 3.7 Imp qt) after engine overhaul.

5. Run the engine for more than 3 minutes then check for oil leakage.