## Automatic Transmission

#### Shift Lever Installation

14-139

4-door Model

1. Install the shift lever assembly.
2. Turn the ignition switch ON (II) and verify that the position indicator light comes on.

3. If necessary, push the shift cable until it stops, then release it. Pull the shift cable back 2 steps so that the shift position is in
4. Turn the ignition switch OFF.

5. Insert a 6.0 mm (0.24 in.) pin (A) through the positioning hole (B) on the shift lever bracket base and into the positioning hole (C) on the shift lever assembly.