## SRS

#### Driver's Airbag Replacement

23-165

Removal

1. Disconnect the battery negative cable and wait at least 3 minutes before beginning work.
2. Remove the access panel (A) from the steering wheel, then disconnect the connector between the cable reel 2P connector (B) and driver's airbag 2P connector (C).

4-door:

5-door:

3. Remove the two Torx bolts (A) using a Torx T30 bit.

Then remove the driver's airbag (B).

4-door:

5-door: