## General Information

#### Body Specifications/Wheel Alignment

1-19

Unit : mm(in.)

*1: With Roof Antenna

*2: European model (MPW condition)

*3: Except European model

Front Wheel Alignment:
Camber | 0°00'±45'
Caster | 1'33'±1°
Total toe | 0±3 (0±0.13)
Wheel turning angle | in | 40°00'±2° (D15B engine) 38°00'±2° (D17A engine)
out | 31°00' (D15B engine: Reference) 30°00' (D17A engine: Reference)

Rear Wheel Alignment:
Camber | -0°45'±45'
Total toe | IN 2 ±3 (0.08 ±0.12)