## Clutch

#### Slave Cylinder Overhaul

12-10

1. ROLL PINS

   Replace

2. BLEEDER SCREW CAP
3. BLEEDER SCREW

   8 Nm (0.8 kgf/m, 5.8 lbf/ft)

4. O-RING

   Replace

5. SLAVE CYLINDER BODY

   Check the cylinder wall for scoring and wear

6. (Brake Assembly Lube)
7. PISTON CLIP

   Replace

8. SLAVE CYLINDER PISTON

   Check for wear and damage.

9. SLAVE CYLINDER SPRING

   Install with small end facing piston.

10. BOOT

    Check that it is fitted securely over the cylinder body.

11. PUSH ROD
12. Urea Grease UM 264

    (P/N 41211-PY-5-305)

13. (Brake Assembly Lube)

a a a