## Automatic Transmission

#### DTC Troubleshooting (cont'd)

14-90

DTC P1713: Problem in D3 Switch Circuit NOTE:

- This DTC is applied to 5-door model.
- Record all freeze data before you troubleshoot.
- The illustration shows the example of connector terminal arrangement; connector terminal arrangement varies with the models.

1. Remove the console panel (see page 20-74).
2. Disconnect the D3 switch connector (6P) on the front of the shift lever bracket.
3. Check for continuity between the No. 2 and No.6 terminals of the D3 switch connector (6P) when the shift lever is in position, then when the shift lever out of position.

D3 SWITCH CONNECTOR (6P)

Terminal side of male terminals

Is there continuity when the shift lever is in position and no continuity when the shift lever out of ?

YES - Go to step 4.

NO - Faulty the D3 switch. Replace the switch.

4. Turn the ignition switch ON (II).

5. Measure the voltage between the No. 6 terminal of the D3 switch connector (6P) and body ground.

D3 SWITCH CONNECTOR (6P)

Wire side of female terminals

Is there 5 V?

YES - Go to step 6.

NO - Repair open or short in the wire between PCM connector terminal B20 and D3 switch connector (6P).

6. Measure the voltage between the No. 2 and No. 6 terminals.

D3 SWITCH CONNECTOR (6P)

Wire side of female terminals

Is there 5 V?

YES - Check for loose terminal fit in the PCM connectors. If necessary, substitute a known-good PCM and recheck.

NO - Repair open in the wire between the No. 2 terminal of D3 switch connector (6P) and ground, or repair poor ground (G401).