## Conventional Brake Components

#### Rear Drum Brake Inspection (cont'd)

19-36

5-door

1. WHEEL CYLINDER

   Inspect for leakage.

2. ADJUSTER BOLT

   Check ratchet teeth for wear and damage.

3. PARKING BRAKE LEVE,

   Marked left and right.

4. UPPER RETURN SPRING

   Check for weakness and damage.

5. WAVE WASHER
6. U-CLIP

   Replace.

7. LOWER RETURN SPRING

   Check for weakness and damage.

8. RETAINER SPRING

   Install securely on tension pin.

9. SELF-ADJUSTER SPRING

   Check for weakness and damage.

10. SELF-ADJUSTER LEVER
11. BRAKE SHOE

    If brake shoes are to be reused, mark and reassemble in the same position.

12. CLEVIS A
13. CLEVIS B
14. 10 mm BOLT

    64 Nm (6.5 kgf/m, 47 lbf/ft)

15. BACKING PLATE

    Marked left and right.

16. TENSION PIN