## Air Conditioning

#### Compressor Clutch Overhaul (cont'd)

21-91

5. Reassemble the clutch in the reverse order of disassembly and note these items:

- Install the field coil with the wire side facing down and align the boss on the field coil with the hole in the compressor.
- Clean the rotor pulley and compressor sliding surfaces with contact cleaner or other non-petroleum solvent.
- Install new snap rings, note the installation direction and make sure they are fully seated in the groove.
- Make sure that the rotor pulley turns smoothly after it is reassembled.
- Route and clamp the wires properly or they can be damaged by the rotor pulley.